

*NIU Construction Standards*

*Division 09 5123 – Acoustical Tile Ceilings*

March 2014, Rev 00









Provide 2 x 2 lay-in system for new installations.

Match existing ceiling system for repairs and renovations. No tile is to be less than 6" in width or length.

Ceiling grid hanger wires to be of adequate strength and quantity to support the tiles and light fixtures. Install tie wires on all four corners of the grid around each fixtures.

Acoustical Tile Ceilings Div 09 5123 Page **1** of **1**